To run the test cases, copy the Par_file, STATIONS and CMTSOLUTION files into the SPECFEM3D_GLOBE/DATA directory.
Recompile the mesher and the solver.
Run the mesher and the solver.
On Curie the commands to put in the submission file are :
ccc_mprun   bin/xmeshfem3D
ccc_mprun   bin/xspecfem3D

SPECFEM3D_TestCaseA runs on 864 cores and SPECFEM3D_TestCaseB runs on 11616 cores.


